CMSIS DSP Software Library: arm_sub_q15.c Source File

- Main Page
- Modules
- Data Structures
- Files
- Examples

- File List
- Globals

# arm_sub_q15.c

Go to the documentation of this file.

    00001 /* ----------------------------------------------------------------------
    00002 * Copyright (C) 2010 ARM Limited. All rights reserved.
    00003 *
    00004 * $Date:        15. July 2011
    00005 * $Revision:    V1.0.10
    00006 *
    00007 * Project:      CMSIS DSP Library
    00008 * Title:        arm_sub_q15.c
    00009 *
    00010 * Description:  Q15 vector subtraction.
    00011 *
    00012 * Target Processor: Cortex-M4/Cortex-M3/Cortex-M0
    00013 *
    00014 * Version 1.0.10 2011/7/15
    00015 *    Big Endian support added and Merged M0 and M3/M4 Source code.
    00016 *
    00017 * Version 1.0.3 2010/11/29
    00018 *    Re-organized the CMSIS folders and updated documentation.
    00019 *
    00020 * Version 1.0.2 2010/11/11
    00021 *    Documentation updated.
    00022 *
    00023 * Version 1.0.1 2010/10/05
    00024 *    Production release and review comments incorporated.
    00025 *
    00026 * Version 1.0.0 2010/09/20
    00027 *    Production release and review comments incorporated.
    00028 *
    00029 * Version 0.0.7  2010/06/10
    00030 *    Misra-C changes done
    00031 * -------------------------------------------------------------------- */
    00032
    00033 #include "arm_math.h"
    00034
    00058 void arm_sub_q15(
    00059   q15_t * pSrcA,
    00060   q15_t * pSrcB,
    00061   q15_t * pDst,
    00062   uint32_t blockSize)
    00063 {
    00064   uint32_t blkCnt;                               /* loop counter */
    00065
    00066
    00067 #ifndef ARM_MATH_CM0
    00068
    00069 /* Run the below code for Cortex-M4 and Cortex-M3 */
    00070   /*loop Unrolling */
    00071   blkCnt = blockSize >> 2u;
    00072
    00073   /* First part of the processing with loop unrolling.  Compute 4 outputs at a time.
    00074    ** a second loop below computes the remaining 1 to 3 samples. */
    00075   while(blkCnt > 0u)
    00076   {
    00077     /* C = A - B */
    00078     /* Subtract and then store the results in the destination buffer two samples at a time. */
    00079     *__SIMD32(pDst)++ = __QSUB16(*__SIMD32(pSrcA)++, *__SIMD32(pSrcB)++);
    00080     *__SIMD32(pDst)++ = __QSUB16(*__SIMD32(pSrcA)++, *__SIMD32(pSrcB)++);
    00081
    00082     /* Decrement the loop counter */
    00083     blkCnt--;
    00084   }
    00085
    00086   /* If the blockSize is not a multiple of 4, compute any remaining output samples here.
    00087    ** No loop unrolling is used. */
    00088   blkCnt = blockSize % 0x4u;
    00089
    00090   while(blkCnt > 0u)
    00091   {
    00092     /* C = A - B */
    00093     /* Subtract and then store the result in the destination buffer. */
    00094     *pDst++ = (q15_t) __QSUB16(*pSrcA++, *pSrcB++);
    00095
    00096     /* Decrement the loop counter */
    00097     blkCnt--;
    00098   }
    00099
    00100 #else
    00101
    00102   /* Run the below code for Cortex-M0 */
    00103
    00104   /* Initialize blkCnt with number of samples */
    00105   blkCnt = blockSize;
    00106
    00107   while(blkCnt > 0u)
    00108   {
    00109     /* C = A - B */
    00110     /* Subtract and then store the result in the destination buffer. */
    00111     *pDst++ = (q15_t) __SSAT(((q31_t) * pSrcA++ - *pSrcB++), 16);
    00112
    00113     /* Decrement the loop counter */
    00114     blkCnt--;
    00115   }
    00116
    00117 #endif /* #ifndef ARM_MATH_CM0 */
    00118
    00119
    00120 }
    00121

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines