CMSIS DSP Software Library: arm_offset_q7.c Source File

- Main Page
- Modules
- Data Structures
- Files
- Examples

- File List
- Globals

# arm_offset_q7.c

Go to the documentation of this file.

    00001 /* ----------------------------------------------------------------------
    00002 * Copyright (C) 2010 ARM Limited. All rights reserved.
    00003 *
    00004 * $Date:        15. July 2011
    00005 * $Revision:    V1.0.10
    00006 *
    00007 * Project:      CMSIS DSP Library
    00008 * Title:        arm_offset_q7.c
    00009 *
    00010 * Description:  Q7 vector offset.
    00011 *
    00012 * Target Processor: Cortex-M4/Cortex-M3/Cortex-M0
    00013 *
    00014 * Version 1.0.10 2011/7/15
    00015 *    Big Endian support added and Merged M0 and M3/M4 Source code.
    00016 *
    00017 * Version 1.0.3 2010/11/29
    00018 *    Re-organized the CMSIS folders and updated documentation.
    00019 *
    00020 * Version 1.0.2 2010/11/11
    00021 *    Documentation updated.
    00022 *
    00023 * Version 1.0.1 2010/10/05
    00024 *    Production release and review comments incorporated.
    00025 *
    00026 * Version 1.0.0 2010/09/20
    00027 *    Production release and review comments incorporated.
    00028 *
    00029 * Version 0.0.7  2010/06/10
    00030 *    Misra-C changes done
    00031 * -------------------------------------------------------------------- */
    00032
    00033 #include "arm_math.h"
    00034
    00058 void arm_offset_q7(
    00059   q7_t * pSrc,
    00060   q7_t offset,
    00061   q7_t * pDst,
    00062   uint32_t blockSize)
    00063 {
    00064   uint32_t blkCnt;                               /* loop counter */
    00065
    00066 #ifndef ARM_MATH_CM0
    00067
    00068 /* Run the below code for Cortex-M4 and Cortex-M3 */
    00069   q31_t offset_packed;                           /* Offset packed to 32 bit */
    00070
    00071
    00072   /*loop Unrolling */
    00073   blkCnt = blockSize >> 2u;
    00074
    00075   /* Offset is packed to 32 bit in order to use SIMD32 for addition */
    00076   offset_packed = __PACKq7(offset, offset, offset, offset);
    00077
    00078   /* First part of the processing with loop unrolling.  Compute 4 outputs at a time.
    00079    ** a second loop below computes the remaining 1 to 3 samples. */
    00080   while(blkCnt > 0u)
    00081   {
    00082     /* C = A + offset */
    00083     /* Add offset and then store the results in the destination bufferfor 4 samples at a time. */
    00084     *__SIMD32(pDst)++ = __QADD8(*__SIMD32(pSrc)++, offset_packed);
    00085
    00086     /* Decrement the loop counter */
    00087     blkCnt--;
    00088   }
    00089
    00090   /* If the blockSize is not a multiple of 4, compute any remaining output samples here.
    00091    ** No loop unrolling is used. */
    00092   blkCnt = blockSize % 0x4u;
    00093
    00094   while(blkCnt > 0u)
    00095   {
    00096     /* C = A + offset */
    00097     /* Add offset and then store the result in the destination buffer. */
    00098     *pDst++ = (q7_t) __SSAT(*pSrc++ + offset, 8);
    00099
    00100     /* Decrement the loop counter */
    00101     blkCnt--;
    00102   }
    00103
    00104 #else
    00105
    00106   /* Run the below code for Cortex-M0 */
    00107
    00108   /* Initialize blkCnt with number of samples */
    00109   blkCnt = blockSize;
    00110
    00111   while(blkCnt > 0u)
    00112   {
    00113     /* C = A + offset */
    00114     /* Add offset and then store the result in the destination buffer. */
    00115     *pDst++ = (q7_t) __SSAT((q15_t) * pSrc++ + offset, 8);
    00116
    00117     /* Decrement the loop counter */
    00118     blkCnt--;
    00119   }
    00120
    00121 #endif /* #ifndef ARM_MATH_CM0 */
    00122
    00123 }
    00124

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines