CMSIS DSP Software Library: Partial Convolution

Functions

# Partial Convolution
[Filtering Functions]

## Functions

arm_status | arm_conv_partial_f32 (float32_t *pSrcA, uint32_t srcALen, float32_t *pSrcB, uint32_t srcBLen, float32_t *pDst, uint32_t firstIndex, uint32_t numPoints)
arm_status | arm_conv_partial_q31 (q31_t *pSrcA, uint32_t srcALen, q31_t *pSrcB, uint32_t srcBLen, q31_t *pDst, uint32_t firstIndex, uint32_t numPoints)
arm_status | arm_conv_partial_fast_q31 (q31_t *pSrcA, uint32_t srcALen, q31_t *pSrcB, uint32_t srcBLen, q31_t *pDst, uint32_t firstIndex, uint32_t numPoints)
arm_status | arm_conv_partial_q15 (q15_t *pSrcA, uint32_t srcALen, q15_t *pSrcB, uint32_t srcBLen, q15_t *pDst, uint32_t firstIndex, uint32_t numPoints)
arm_status | arm_conv_partial_fast_q15 (q15_t *pSrcA, uint32_t srcALen, q15_t *pSrcB, uint32_t srcBLen, q15_t *pDst, uint32_t firstIndex, uint32_t numPoints)
arm_status | arm_conv_partial_q7 (q7_t *pSrcA, uint32_t srcALen, q7_t *pSrcB, uint32_t srcBLen, q7_t *pDst, uint32_t firstIndex, uint32_t numPoints)

## Detailed Description

Partial Convolution is equivalent to Convolution except that a subset of the output samples is generated. Each function has two additional arguments. `firstIndex` specifies the starting index of the subset of output samples. `numPoints` is the number of output samples to compute. The function computes the output in the range `[firstIndex, ..., firstIndex+numPoints-1]`. The output array `pDst` contains `numPoints` values.

The allowable range of output indices is [0 srcALen+srcBLen-2]. If the requested subset does not fall in this range then the functions return ARM_MATH_ARGUMENT_ERROR. Otherwise the functions return ARM_MATH_SUCCESS.

Note:
  Refer arm_conv_f32() for details on fixed point behavior.

## Function Documentation

arm_status arm_conv_partial_f32 | ( | float32_t * | pSrcA,
|  | uint32_t | srcALen,
|  | float32_t * | pSrcB,
|  | uint32_t | srcBLen,
|  | float32_t * | pDst,
|  | uint32_t | firstIndex,
|  | uint32_t | numPoints
| ) |  |

Partial convolution of floating-point sequences.

Parameters:

  [in] | *pSrcA | points to the first input sequence.
  [in] | srcALen | length of the first input sequence.
  [in] | *pSrcB | points to the second input sequence.
  [in] | srcBLen | length of the second input sequence.
  [out] | *pDst | points to the location where the output result is written.
  [in] | firstIndex | is the first output sample to start with.
  [in] | numPoints | is the number of output points to be computed.

Returns:
  Returns either ARM_MATH_SUCCESS if the function completed correctly or ARM_MATH_ARGUMENT_ERROR if the requested subset is not in the range [0 srcALen+srcBLen-2].

Definition at line 74 of file arm_conv_partial_f32.c.

arm_status arm_conv_partial_q31 | ( | q31_t * | pSrcA,
|  | uint32_t | srcALen,
|  | q31_t * | pSrcB,
|  | uint32_t | srcBLen,
|  | q31_t * | pDst,
|  | uint32_t | firstIndex,
|  | uint32_t | numPoints
| ) |  |

Partial convolution of Q31 sequences.

Parameters:

  [in] | *pSrcA | points to the first input sequence.
  [in] | srcALen | length of the first input sequence.
  [in] | *pSrcB | points to the second input sequence.
  [in] | srcBLen | length of the second input sequence.
  [out] | *pDst | points to the location where the output result is written.
  [in] | firstIndex | is the first output sample to start with.
  [in] | numPoints | is the number of output points to be computed.

Returns:
  Returns either ARM_MATH_SUCCESS if the function completed correctly or ARM_MATH_ARGUMENT_ERROR if the requested subset is not in the range [0 srcALen+srcBLen-2].

See `arm_conv_partial_fast_q31()` for a faster but less precise implementation of this function for Cortex-M3 and Cortex-M4.

Definition at line 59 of file arm_conv_partial_q31.c.

arm_status arm_conv_partial_fast_q31 | ( | q31_t * | pSrcA,
|  | uint32_t | srcALen,
|  | q31_t * | pSrcB,
|  | uint32_t | srcBLen,
|  | q31_t * | pDst,
|  | uint32_t | firstIndex,
|  | uint32_t | numPoints
| ) |  |

Partial convolution of Q31 sequences (fast version) for Cortex-M3 and Cortex-M4.

Parameters:

  [in] | *pSrcA | points to the first input sequence.
  [in] | srcALen | length of the first input sequence.
  [in] | *pSrcB | points to the second input sequence.
  [in] | srcBLen | length of the second input sequence.
  [out] | *pDst | points to the location where the output result is written.
  [in] | firstIndex | is the first output sample to start with.
  [in] | numPoints | is the number of output points to be computed.

Returns:
  Returns either ARM_MATH_SUCCESS if the function completed correctly or ARM_MATH_ARGUMENT_ERROR if the requested subset is not in the range [0 srcALen+srcBLen-2].

  See `arm_conv_partial_q31()` for a slower implementation of this function which uses a 64-bit accumulator to provide higher precision.

Definition at line 56 of file arm_conv_partial_fast_q31.c.

arm_status arm_conv_partial_q15 | ( | q15_t * | pSrcA,
|  | uint32_t | srcALen,
|  | q15_t * | pSrcB,
|  | uint32_t | srcBLen,
|  | q15_t * | pDst,
|  | uint32_t | firstIndex,
|  | uint32_t | numPoints
| ) |  |

Partial convolution of Q15 sequences.

Parameters:

  [in] | *pSrcA | points to the first input sequence.
  [in] | srcALen | length of the first input sequence.
  [in] | *pSrcB | points to the second input sequence.
  [in] | srcBLen | length of the second input sequence.
  [out] | *pDst | points to the location where the output result is written.
  [in] | firstIndex | is the first output sample to start with.
  [in] | numPoints | is the number of output points to be computed.

Returns:
  Returns either ARM_MATH_SUCCESS if the function completed correctly or ARM_MATH_ARGUMENT_ERROR if the requested subset is not in the range [0 srcALen+srcBLen-2].

Refer to `arm_conv_partial_fast_q15()` for a faster but less precise version of this function for Cortex-M3 and Cortex-M4.

Definition at line 60 of file arm_conv_partial_q15.c.

arm_status arm_conv_partial_fast_q15 | ( | q15_t * | pSrcA,
|  | uint32_t | srcALen,
|  | q15_t * | pSrcB,
|  | uint32_t | srcBLen,
|  | q15_t * | pDst,
|  | uint32_t | firstIndex,
|  | uint32_t | numPoints
| ) |  |

Partial convolution of Q15 sequences (fast version) for Cortex-M3 and Cortex-M4.

Parameters:

  [in] | *pSrcA | points to the first input sequence.
  [in] | srcALen | length of the first input sequence.
  [in] | *pSrcB | points to the second input sequence.
  [in] | srcBLen | length of the second input sequence.
  [out] | *pDst | points to the location where the output result is written.
  [in] | firstIndex | is the first output sample to start with.
  [in] | numPoints | is the number of output points to be computed.

Returns:
  Returns either ARM_MATH_SUCCESS if the function completed correctly or ARM_MATH_ARGUMENT_ERROR if the requested subset is not in the range [0 srcALen+srcBLen-2].

See `arm_conv_partial_q15()` for a slower implementation of this function which uses a 64-bit accumulator to avoid wrap around distortion.

Definition at line 56 of file arm_conv_partial_fast_q15.c.

arm_status arm_conv_partial_q7 | ( | q7_t * | pSrcA,
|  | uint32_t | srcALen,
|  | q7_t * | pSrcB,
|  | uint32_t | srcBLen,
|  | q7_t * | pDst,
|  | uint32_t | firstIndex,
|  | uint32_t | numPoints
| ) |  |

Partial convolution of Q7 sequences.

Parameters:

  [in] | *pSrcA | points to the first input sequence.
  [in] | srcALen | length of the first input sequence.
  [in] | *pSrcB | points to the second input sequence.
  [in] | srcBLen | length of the second input sequence.
  [out] | *pDst | points to the location where the output result is written.
  [in] | firstIndex | is the first output sample to start with.
  [in] | numPoints | is the number of output points to be computed.

Returns:
  Returns either ARM_MATH_SUCCESS if the function completed correctly or ARM_MATH_ARGUMENT_ERROR if the requested subset is not in the range [0 srcALen+srcBLen-2].

Definition at line 58 of file arm_conv_partial_q7.c.

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines