Static Call Graph - [.\Output\Discovery.axf]

# Static Call Graph for image .\Output\Discovery.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 76]: Last Updated: Mon Mar 17 00:46:13 2014

### Maximum Stack Usage = 172 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ OV9655_Configuration ⇒ OV9655_DCMI_Configuration ⇒ DMA_DeInit

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - BusFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - CRYP_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DCMI_IRQHandler from stm32f4xx_it.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - ETH_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - EXTI9_5_IRQHandler from touch_7846.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - FPU_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - FSMC_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - HASH_RNG_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - PVD_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - RCC_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - Reset_Handler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - SDIO_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - SVC_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - SystemInit from system_stm32f4xx.o(.text) referenced from startup_stm32f40xx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - UART4_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - UART5_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - USART1_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - USART2_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - USART3_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - USART6_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - UsageFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f40xx.o(.text) referenced from startup_stm32f40xx.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f40xx.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000001))
  [Calls]

  - >> _fp_init

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000031))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 172 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ OV9655_Configuration ⇒ OV9655_DCMI_Configuration ⇒ DMA_DeInit
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f40xx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  CRYP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f40xx.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  main (Thumb, 150 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 172
  - Call Chain = main ⇒ OV9655_Configuration ⇒ OV9655_DCMI_Configuration ⇒ DMA_DeInit
  [Calls]
  - >> STM_EVAL_LEDInit
  - >> STM3240F_LCD_Init
  - >> OV9655_Configuration
  - >> LCD_WriteRAM_Prepare
  - >> LCD_SetFont
  - >> LCD_SetDisplayWindow
  - >> LCD_SetColors
  - >> LCD_DisplayStringLine
  - >> LCD_Clear
  - >> DMA_Cmd
  - >> DCMI_Cmd
  - >> DCMI_CaptureCmd
  - >> SystemInit
  [Called By]
  - >> __rt_entry_main

  Delay (Thumb, 16 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Delay
  [Called By]
  - >> DCMI_OV9655_QQVGASizeSetup
  - >> DCMI_OV9655_QVGASizeSetup

  TimingDelay_Decrement (Thumb, 16 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> SysTick_Handler

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f40xx.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f40xx.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f40xx.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f40xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40xx.o(RESET)

  SysTick_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> TimingDelay_Decrement
  [Address Reference Count : 1]
  - startup_stm32f40xx.o(RESET)

  DCMI_IRQHandler (Thumb, 90 bytes, Stack size 8 bytes, stm32f4xx_it.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = DCMI_IRQHandler ⇒ LCD_SetDisplayWindow ⇒ LCD_SetCursor
  [Calls]
  - >> STM_EVAL_LEDToggle
  - >> DCMI_GetITStatus
  - >> DCMI_ClearITPendingBit
  - >> LCD_WriteRAM_Prepare
  - >> LCD_SetDisplayWindow
  [Address Reference Count : 1]
  - startup_stm32f40xx.o(RESET)

  SystemInit (Thumb, 82 bytes, Stack size 8 bytes, system_stm32f4xx.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Called By]
  - >> main
  [Address Reference Count : 1]
  - startup_stm32f40xx.o(.text)

  SystemCoreClockUpdate (Thumb, 108 bytes, Stack size 16 bytes, system_stm32f4xx.o(.text), UNUSED)

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> OV9655_DCMI_Configuration
  - >> NVIC_TOUCHConfiguration

  NVIC_Init (Thumb, 92 bytes, Stack size 16 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> OV9655_DCMI_Configuration
  - >> touch_init
  - >> NVIC_TOUCHConfiguration
  - >> STM_EVAL_PBInit

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)
  [Called By]

  - >> NVIC_TOUCHConfiguration

  NVIC_SystemLPConfig (Thumb, 20 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  DCMI_DeInit (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(.text), UNUSED)

  DCMI_Init (Thumb, 54 bytes, Stack size 12 bytes, stm32f4xx_dcmi.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = DCMI_Init
  [Called By]
  - >> OV9655_DCMI_Configuration

  DCMI_StructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(.text), UNUSED)

  DCMI_CROPConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(.text), UNUSED)

  DCMI_CROPCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(.text), UNUSED)

  DCMI_SetEmbeddedSynchroCodes (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(.text), UNUSED)

  DCMI_JPEGCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(.text), UNUSED)

  DCMI_Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(.text))
  [Called By]

  - >> main

  DCMI_CaptureCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(.text))
  [Called By]

  - >> main

  DCMI_ReadData (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(.text), UNUSED)

  DCMI_ITConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(.text))
  [Called By]

  - >> OV9655_DCMI_Configuration

  DCMI_GetFlagStatus (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(.text), UNUSED)

  DCMI_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(.text), UNUSED)

  DCMI_GetITStatus (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(.text))
  [Called By]

  - >> DCMI_IRQHandler

  DCMI_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(.text))
  [Called By]

  - >> DCMI_IRQHandler

  DMA_DeInit (Thumb, 272 bytes, Stack size 28 bytes, stm32f4xx_dma.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = DMA_DeInit
  [Called By]
  - >> OV9655_DCMI_Configuration

  DMA_Init (Thumb, 80 bytes, Stack size 12 bytes, stm32f4xx_dma.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = DMA_Init
  [Called By]
  - >> OV9655_DCMI_Configuration

  DMA_StructInit (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text))
  [Called By]

  - >> main

  DMA_PeriphIncOffsetSizeConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_FlowControllerConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_SetCurrDataCounter (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetCurrDataCounter (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_DoubleBufferModeConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_DoubleBufferModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_MemoryTargetConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetCurrentMemoryTarget (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetCmdStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetFIFOStatus (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetFlagStatus (Thumb, 42 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_ClearFlag (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_ITConfig (Thumb, 52 bytes, Stack size 8 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetITStatus (Thumb, 70 bytes, Stack size 12 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_ClearITPendingBit (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  EXTI_DeInit (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_Init (Thumb, 108 bytes, Stack size 12 bytes, stm32f4xx_exti.o(.text), UNUSED)
  [Called By]

  - >> touch_init
  - >> STM_EVAL_PBInit

  EXTI_StructInit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_GenerateSWInterrupt (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_ClearFlag (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_GetITStatus (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text))
  [Called By]

  - >> EXTI9_5_IRQHandler

  EXTI_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text))
  [Called By]

  - >> EXTI9_5_IRQHandler

  FSMC_NORSRAMDeInit (Thumb, 36 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NORSRAMInit (Thumb, 192 bytes, Stack size 12 bytes, stm32f4xx_fsmc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = FSMC_NORSRAMInit
  [Called By]
  - >> LCD_FSMCConfig

  FSMC_NORSRAMStructInit (Thumb, 98 bytes, Stack size 8 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NORSRAMCmd (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text))
  [Called By]

  - >> LCD_FSMCConfig

  FSMC_NANDDeInit (Thumb, 40 bytes, Stack size 8 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NANDInit (Thumb, 104 bytes, Stack size 12 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NANDStructInit (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NANDCmd (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NANDECCCmd (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_GetECC (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_PCCARDDeInit (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_PCCARDInit (Thumb, 98 bytes, Stack size 8 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_PCCARDStructInit (Thumb, 60 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_PCCARDCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_ITConfig (Thumb, 68 bytes, Stack size 8 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_GetFlagStatus (Thumb, 40 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_ClearFlag (Thumb, 36 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_GetITStatus (Thumb, 48 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_ClearITPendingBit (Thumb, 40 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  GPIO_DeInit (Thumb, 192 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_AHB1PeriphResetCmd

  GPIO_Init (Thumb, 162 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> STM_EVAL_LEDInit
  - >> Soft_I2C_Configuration
  - >> OV9655_MCO_Configuration
  - >> OV9655_DCMI_Configuration
  - >> touch_init
  - >> LCD_CtrlLinesConfig
  - >> STM_EVAL_PBInit

  GPIO_StructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 24 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text))
  [Called By]

  - >> I2C_WaitAck
  - >> I2C_ReceiveByte
  - >> Read_Ads7846
  - >> STM_EVAL_PBGetState

  GPIO_ReadInputData (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text))
  [Called By]

  - >> I2C_WaitAck
  - >> I2C_Stop
  - >> I2C_Start
  - >> I2C_SendByte
  - >> I2C_ReceiveByte
  - >> touch_init
  - >> TPReadY
  - >> TPReadX
  - >> I2C_NoAck
  - >> I2C_Ack

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text))
  [Called By]

  - >> I2C_WaitAck
  - >> I2C_Stop
  - >> I2C_Start
  - >> I2C_SendByte
  - >> I2C_ReceiveByte
  - >> TPReadY
  - >> TPReadX
  - >> I2C_NoAck
  - >> I2C_Ack

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ToggleBits (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinAFConfig (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = GPIO_PinAFConfig
  [Called By]
  - >> OV9655_MCO_Configuration
  - >> OV9655_DCMI_Configuration
  - >> touch_init
  - >> LCD_CtrlLinesConfig

  RCC_DeInit (Thumb, 48 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 46 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> OV9655_MCO_Configuration
  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 44 bytes, Stack size 12 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> OV9655_MCO_Configuration

  RCC_PLLI2SCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> OV9655_MCO_Configuration

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO1Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO2Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> OV9655_MCO_Configuration

  RCC_SYSCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 134 bytes, Stack size 16 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 42 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_I2SCLKConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB1PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> STM_EVAL_LEDInit
  - >> Soft_I2C_Configuration
  - >> OV9655_MCO_Configuration
  - >> OV9655_DCMI_Configuration
  - >> touch_init
  - >> LCD_CtrlLinesConfig
  - >> STM_EVAL_PBInit

  RCC_AHB2PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> OV9655_DCMI_Configuration

  RCC_AHB3PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> LCD_FSMCConfig

  RCC_APB1PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> touch_init

  RCC_APB2PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> touch_init
  - >> LCD_FSMCConfig
  - >> STM_EVAL_PBInit

  RCC_AHB1PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> GPIO_DeInit

  RCC_AHB2PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> SPI_I2S_DeInit

  RCC_APB2PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> SYSCFG_DeInit
  - >> SPI_I2S_DeInit

  RCC_AHB1PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB2PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  SPI_I2S_DeInit (Thumb, 72 bytes, Stack size 8 bytes, stm32f4xx_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd
  [Called By]
  - >> touch_init

  SPI_Init (Thumb, 56 bytes, Stack size 12 bytes, stm32f4xx_spi.o(.text), UNUSED)
  [Called By]

  - >> touch_init

  I2S_Init (Thumb, 190 bytes, Stack size 20 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  I2S_StructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)
  [Called By]

  - >> touch_init

  I2S_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_DataSizeConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_BiDirectionalLineConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_NSSInternalSoftwareConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_SSOutputCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_TIModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  I2S_FullDuplexConfig (Thumb, 58 bytes, Stack size 12 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_ReceiveData (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text))
  [Called By]

  - >> SPI_WriteByte

  SPI_I2S_SendData (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text))
  [Called By]

  - >> SPI_WriteByte

  SPI_CalculateCRC (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_TransmitCRC (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_GetCRC (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_GetCRCPolynomial (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_DMACmd (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_ITConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text))
  [Called By]

  - >> SPI_WriteByte

  SPI_I2S_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_GetITStatus (Thumb, 42 bytes, Stack size 8 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_ClearITPendingBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SYSCFG_DeInit (Thumb, 24 bytes, Stack size 8 bytes, stm32f4xx_syscfg.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  SYSCFG_MemoryRemapConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_syscfg.o(.text), UNUSED)

  SYSCFG_EXTILineConfig (Thumb, 36 bytes, Stack size 8 bytes, stm32f4xx_syscfg.o(.text), UNUSED)
  [Called By]

  - >> touch_init
  - >> STM_EVAL_PBInit

  SYSCFG_ETH_MediaInterfaceConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_syscfg.o(.text), UNUSED)

  SYSCFG_CompensationCellCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_syscfg.o(.text), UNUSED)

  SYSCFG_GetCompensationCellStatus (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_syscfg.o(.text), UNUSED)

  STM_EVAL_LEDInit (Thumb, 62 bytes, Stack size 16 bytes, stm32f4_discovery.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = STM_EVAL_LEDInit ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> main

  STM_EVAL_LEDOn (Thumb, 18 bytes, Stack size 0 bytes, stm32f4_discovery.o(.text), UNUSED)

  STM_EVAL_LEDOff (Thumb, 18 bytes, Stack size 0 bytes, stm32f4_discovery.o(.text), UNUSED)

  STM_EVAL_LEDToggle (Thumb, 22 bytes, Stack size 0 bytes, stm32f4_discovery.o(.text))
  [Called By]

  - >> DCMI_IRQHandler

  STM_EVAL_PBInit (Thumb, 148 bytes, Stack size 40 bytes, stm32f4_discovery.o(.text), UNUSED)
  [Calls]

  - >> GPIO_Init
  - >> EXTI_Init
  - >> NVIC_Init
  - >> SYSCFG_EXTILineConfig
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd

  STM_EVAL_PBGetState (Thumb, 20 bytes, Stack size 0 bytes, stm32f4_discovery.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ReadInputDataBit

  LCD_SetFont (Thumb, 6 bytes, Stack size 0 bytes, stm3240f_lcd.o(.text))
  [Called By]

  - >> main

  LCD_WriteReg (Thumb, 12 bytes, Stack size 0 bytes, stm3240f_lcd.o(.text))
  [Called By]

  - >> STM3240F_LCD_Init
  - >> LCD_SetDisplayWindow
  - >> LCD_DisplayOff
  - >> LCD_DisplayOn
  - >> LCD_PowerOn
  - >> LCD_WriteBMP
  - >> LCD_WindowModeDisable
  - >> LCD_SetCursor

  LCD_FSMCConfig (Thumb, 98 bytes, Stack size 96 bytes, stm3240f_lcd.o(.text))
  [Stack]

  - Max Depth = 108
  - Call Chain = LCD_FSMCConfig ⇒ FSMC_NORSRAMInit
  [Calls]
  - >> FSMC_NORSRAMCmd
  - >> FSMC_NORSRAMInit
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB3PeriphClockCmd
  [Called By]
  - >> STM3240F_LCD_Init

  LCD_CtrlLinesConfig (Thumb, 288 bytes, Stack size 24 bytes, stm3240f_lcd.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = LCD_CtrlLinesConfig ⇒ GPIO_Init
  [Calls]
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> STM3240F_LCD_Init

  STM3240F_LCD_Init (Thumb, 454 bytes, Stack size 16 bytes, stm3240f_lcd.o(.text))
  [Stack]

  - Max Depth = 124
  - Call Chain = STM3240F_LCD_Init ⇒ LCD_FSMCConfig ⇒ FSMC_NORSRAMInit
  [Calls]
  - >> LCD_CtrlLinesConfig
  - >> LCD_FSMCConfig
  - >> LCD_WriteReg
  - >> delay
  [Called By]
  - >> main

  LCD_SetColors (Thumb, 18 bytes, Stack size 12 bytes, stm3240f_lcd.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = LCD_SetColors
  [Called By]
  - >> main

  LCD_GetColors (Thumb, 12 bytes, Stack size 0 bytes, stm3240f_lcd.o(.text), UNUSED)

  LCD_SetTextColor (Thumb, 12 bytes, Stack size 8 bytes, stm3240f_lcd.o(.text), UNUSED)

  LCD_SetBackColor (Thumb, 12 bytes, Stack size 8 bytes, stm3240f_lcd.o(.text), UNUSED)

  LCD_GetFont (Thumb, 6 bytes, Stack size 0 bytes, stm3240f_lcd.o(.text), UNUSED)

  LCD_WriteRAM (Thumb, 6 bytes, Stack size 0 bytes, stm3240f_lcd.o(.text), UNUSED)

  LCD_WriteRAM_Prepare (Thumb, 10 bytes, Stack size 0 bytes, stm3240f_lcd.o(.text))
  [Called By]

  - >> DCMI_IRQHandler
  - >> main

  LCD_SetCursor (Thumb, 28 bytes, Stack size 4 bytes, stm3240f_lcd.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = LCD_SetCursor
  [Calls]
  - >> LCD_WriteReg
  [Called By]
  - >> LCD_SetDisplayWindow
  - >> LCD_DrawCircle
  - >> LCD_GetPixel
  - >> LCD_PutPixel
  - >> LCD_DrawChar

  LCD_DrawChar (Thumb, 134 bytes, Stack size 28 bytes, stm3240f_lcd.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = LCD_DrawChar ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_SetCursor
  [Called By]
  - >> LCD_DisplayChar

  LCD_DisplayChar (Thumb, 24 bytes, Stack size 4 bytes, stm3240f_lcd.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = LCD_DisplayChar ⇒ LCD_DrawChar ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_DrawChar
  [Called By]
  - >> LCD_DisplayStringLine
  - >> LCD_ShowNum
  - >> LCD_ClearLine

  LCD_ClearLine (Thumb, 44 bytes, Stack size 16 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_DisplayChar

  LCD_Clear (Thumb, 26 bytes, Stack size 0 bytes, stm3240f_lcd.o(.text))
  [Called By]

  - >> main

  LCD_DisplayStringLine (Thumb, 58 bytes, Stack size 24 bytes, stm3240f_lcd.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = LCD_DisplayStringLine ⇒ LCD_DisplayChar ⇒ LCD_DrawChar ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_DisplayChar
  [Called By]
  - >> main

  LCD_SetDisplayWindow (Thumb, 44 bytes, Stack size 16 bytes, stm3240f_lcd.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = LCD_SetDisplayWindow ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_SetCursor
  - >> LCD_WriteReg
  [Called By]
  - >> DCMI_IRQHandler
  - >> main
  - >> LCD_DrawFullRect
  - >> LCD_WriteBMP2

  LCD_PutPixel (Thumb, 14 bytes, Stack size 8 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_SetCursor
  [Called By]
  - >> LCD_FillPolyLine
  - >> LCD_DrawFullRect
  - >> LCD_DrawLine

  LCD_ReadRAM (Thumb, 14 bytes, Stack size 0 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Called By]

  - >> LCD_GetPixel

  LCD_GetPixel (Thumb, 12 bytes, Stack size 4 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_ReadRAM
  - >> LCD_SetCursor

  LCD_WindowModeDisable (Thumb, 8 bytes, Stack size 0 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_WriteReg

  LCD_DrawLine (Thumb, 188 bytes, Stack size 48 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_PutPixel
  [Called By]
  - >> LCD_FillPolyLine
  - >> LCD_ClosedPolyLine
  - >> LCD_PolyLine
  - >> LCD_DrawFullCircle
  - >> LCD_Rectangle
  - >> LCD_PolyLineRelativeClosed

  LCD_Rectangle (Thumb, 54 bytes, Stack size 20 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_DrawLine

  LCD_DrawCircle (Thumb, 282 bytes, Stack size 48 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_SetCursor

  LCD_DrawMonoPict (Thumb, 58 bytes, Stack size 20 bytes, stm3240f_lcd.o(.text), UNUSED)

  LCD_WriteBMP (Thumb, 74 bytes, Stack size 8 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_WriteReg

  LCD_WriteBMP2 (Thumb, 56 bytes, Stack size 12 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_SetDisplayWindow

  LCD_DrawFullRect (Thumb, 108 bytes, Stack size 24 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_SetDisplayWindow
  - >> LCD_PutPixel

  LCD_DrawFullCircle (Thumb, 144 bytes, Stack size 32 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_DrawLine

  LCD_PolyLine (Thumb, 40 bytes, Stack size 12 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_DrawLine
  [Called By]
  - >> LCD_ClosedPolyLine

  LCD_ClosedPolyLine (Thumb, 30 bytes, Stack size 12 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_PolyLine
  - >> LCD_DrawLine

  LCD_PolyLineRelative (Thumb, 4 bytes, Stack size 0 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_PolyLineRelativeClosed

  LCD_ClosedPolyLineRelative (Thumb, 4 bytes, Stack size 0 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_PolyLineRelativeClosed

  LCD_FillPolyLine (Thumb, 486 bytes, Stack size 456 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_DrawLine
  - >> LCD_PutPixel
  - >> __aeabi_cdrcmple
  - >> __aeabi_cdcmple
  - >> __aeabi_ui2d
  - >> __aeabi_i2d

  LCD_ReadReg (Thumb, 6 bytes, Stack size 0 bytes, stm3240f_lcd.o(.text), UNUSED)

  LCD_PowerOn (Thumb, 120 bytes, Stack size 8 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_WriteReg
  - >> delay

  LCD_DisplayOn (Thumb, 10 bytes, Stack size 0 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_WriteReg

  LCD_DisplayOff (Thumb, 8 bytes, Stack size 0 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_WriteReg

  SPI_WriteByte (Thumb, 48 bytes, Stack size 16 bytes, touch_7846.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SPI_WriteByte
  [Calls]
  - >> SPI_I2S_GetFlagStatus
  - >> SPI_I2S_SendData
  - >> SPI_I2S_ReceiveData
  [Called By]
  - >> TPReadY
  - >> TPReadX

  SpiDelay (Thumb, 12 bytes, Stack size 0 bytes, touch_7846.o(.text))
  [Called By]

  - >> TPReadY
  - >> TPReadX

  TPReadX (Thumb, 72 bytes, Stack size 16 bytes, touch_7846.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = TPReadX ⇒ SPI_WriteByte
  [Calls]
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> SpiDelay
  - >> SPI_WriteByte
  [Called By]
  - >> read_once

  TPReadY (Thumb, 66 bytes, Stack size 16 bytes, touch_7846.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = TPReadY ⇒ SPI_WriteByte
  [Calls]
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> SpiDelay
  - >> SPI_WriteByte
  [Called By]
  - >> read_once

  read_once (Thumb, 20 bytes, Stack size 8 bytes, touch_7846.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = read_once ⇒ TPReadY ⇒ SPI_WriteByte
  [Calls]
  - >> TPReadY
  - >> TPReadX
  [Called By]
  - >> Read_Ads7846

  NVIC_TOUCHConfiguration (Thumb, 46 bytes, Stack size 8 bytes, touch_7846.o(.text), UNUSED)
  [Calls]

  - >> NVIC_SetVectorTable
  - >> NVIC_Init
  - >> NVIC_PriorityGroupConfig

  touch_init (Thumb, 292 bytes, Stack size 64 bytes, touch_7846.o(.text), UNUSED)
  [Calls]

  - >> GPIO_PinAFConfig
  - >> GPIO_SetBits
  - >> GPIO_Init
  - >> EXTI_Init
  - >> NVIC_Init
  - >> SYSCFG_EXTILineConfig
  - >> SPI_Cmd
  - >> SPI_Init
  - >> SPI_I2S_DeInit
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd

  LCD_ShowNum (Thumb, 152 bytes, Stack size 24 bytes, touch_7846.o(.text), UNUSED)
  [Calls]

  - >> LCD_DisplayChar

  Read_Ads7846 (Thumb, 222 bytes, Stack size 64 bytes, touch_7846.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = Read_Ads7846 ⇒ read_once ⇒ TPReadY ⇒ SPI_WriteByte
  [Calls]
  - >> GPIO_ReadInputDataBit
  - >> read_once
  [Called By]
  - >> EXTI9_5_IRQHandler

  EXTI9_5_IRQHandler (Thumb, 26 bytes, Stack size 8 bytes, touch_7846.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = EXTI9_5_IRQHandler ⇒ Read_Ads7846 ⇒ read_once ⇒ TPReadY ⇒ SPI_WriteByte
  [Calls]
  - >> EXTI_ClearITPendingBit
  - >> EXTI_GetITStatus
  - >> Read_Ads7846
  [Address Reference Count : 1]
  - startup_stm32f40xx.o(RESET)

  OV9655_DCMI_Configuration (Thumb, 376 bytes, Stack size 128 bytes, ov9655.o(.text))
  [Stack]

  - Max Depth = 156
  - Call Chain = OV9655_DCMI_Configuration ⇒ DMA_DeInit
  [Calls]
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> DMA_Init
  - >> DMA_DeInit
  - >> DCMI_ITConfig
  - >> DCMI_Init
  - >> NVIC_Init
  - >> NVIC_PriorityGroupConfig
  - >> RCC_AHB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> OV9655_Configuration

  DCMI_SingleRandomWrite (Thumb, 66 bytes, Stack size 16 bytes, ov9655.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = DCMI_SingleRandomWrite ⇒ I2C_SendByte
  [Calls]
  - >> I2C_WaitAck
  - >> I2C_Stop
  - >> I2C_Start
  - >> I2C_SendByte
  - >> I2C_Delay
  [Called By]
  - >> OV9655_Configuration
  - >> DCMI_OV9655_SelectRGBOption
  - >> DCMI_OV9655_HREFControl
  - >> DCMI_OV9655_SetRegister
  - >> DCMI_OV9655_SelectFormatResolution
  - >> DCMI_OV9655_SelectOutputFormat
  - >> DCMI_OV9655_SetPrescaler
  - >> DCMI_OV9655_QQVGASizeSetup
  - >> DCMI_OV9655_Reset
  - >> DCMI_OV9655_QVGASizeSetup

  DCMI_OV9655_QVGASizeSetup (Thumb, 3050 bytes, Stack size 8 bytes, ov9655.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = DCMI_OV9655_QVGASizeSetup ⇒ DCMI_SingleRandomWrite ⇒ I2C_SendByte
  [Calls]
  - >> Delay
  - >> DCMI_SingleRandomWrite
  [Called By]
  - >> OV9655_Configuration

  DCMI_SingleRandomRead (Thumb, 80 bytes, Stack size 16 bytes, ov9655.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = DCMI_SingleRandomRead ⇒ I2C_ReceiveByte
  [Calls]
  - >> I2C_WaitAck
  - >> I2C_Stop
  - >> I2C_Start
  - >> I2C_SendByte
  - >> I2C_ReceiveByte
  - >> I2C_Delay
  [Called By]
  - >> DCMI_OV9655_ReadID

  DCMI_OV9655_ReadID (Thumb, 46 bytes, Stack size 8 bytes, ov9655.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = DCMI_OV9655_ReadID ⇒ DCMI_SingleRandomRead ⇒ I2C_ReceiveByte
  [Calls]
  - >> DCMI_SingleRandomRead
  [Called By]
  - >> OV9655_Configuration

  OV9655_MCO_Configuration (Thumb, 98 bytes, Stack size 16 bytes, ov9655.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = OV9655_MCO_Configuration ⇒ GPIO_Init
  [Calls]
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> RCC_AHB1PeriphClockCmd
  - >> RCC_MCO2Config
  - >> RCC_PLLI2SCmd
  - >> RCC_PLLI2SConfig
  - >> RCC_GetFlagStatus
  [Called By]
  - >> OV9655_Configuration

  OV9655_Configuration (Thumb, 92 bytes, Stack size 16 bytes, ov9655.o(.text))
  [Stack]

  - Max Depth = 172
  - Call Chain = OV9655_Configuration ⇒ OV9655_DCMI_Configuration ⇒ DMA_DeInit
  [Calls]
  - >> Soft_I2C_Configuration
  - >> OV9655_MCO_Configuration
  - >> DCMI_OV9655_ReadID
  - >> DCMI_OV9655_QVGASizeSetup
  - >> DCMI_SingleRandomWrite
  - >> OV9655_DCMI_Configuration
  [Called By]
  - >> main

  DCMI_OV9655_Reset (Thumb, 10 bytes, Stack size 0 bytes, ov9655.o(.text), UNUSED)
  [Calls]

  - >> DCMI_SingleRandomWrite

  DCMI_OV9655_QQVGASizeSetup (Thumb, 2402 bytes, Stack size 8 bytes, ov9655.o(.text), UNUSED)
  [Calls]

  - >> Delay
  - >> DCMI_SingleRandomWrite

  DCMI_OV9655_SetPrescaler (Thumb, 10 bytes, Stack size 0 bytes, ov9655.o(.text), UNUSED)
  [Calls]

  - >> DCMI_SingleRandomWrite

  DCMI_OV9655_SelectOutputFormat (Thumb, 10 bytes, Stack size 0 bytes, ov9655.o(.text), UNUSED)
  [Calls]

  - >> DCMI_SingleRandomWrite

  DCMI_OV9655_SelectFormatResolution (Thumb, 10 bytes, Stack size 0 bytes, ov9655.o(.text), UNUSED)
  [Calls]

  - >> DCMI_SingleRandomWrite

  DCMI_OV9655_SetRegister (Thumb, 10 bytes, Stack size 0 bytes, ov9655.o(.text), UNUSED)
  [Calls]

  - >> DCMI_SingleRandomWrite

  DCMI_OV9655_HREFControl (Thumb, 10 bytes, Stack size 0 bytes, ov9655.o(.text), UNUSED)
  [Calls]

  - >> DCMI_SingleRandomWrite

  DCMI_OV9655_SelectRGBOption (Thumb, 10 bytes, Stack size 0 bytes, ov9655.o(.text), UNUSED)
  [Calls]

  - >> DCMI_SingleRandomWrite

  Soft_I2C_Configuration (Thumb, 86 bytes, Stack size 24 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = Soft_I2C_Configuration ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> OV9655_Configuration

  I2C_Delay (Thumb, 10 bytes, Stack size 0 bytes, i2c.o(.text))
  [Called By]

  - >> I2C_WaitAck
  - >> I2C_Stop
  - >> I2C_Start
  - >> I2C_SendByte
  - >> I2C_ReceiveByte
  - >> DCMI_SingleRandomRead
  - >> DCMI_SingleRandomWrite
  - >> I2C_NoAck
  - >> I2C_Ack

  I2C_Start (Thumb, 58 bytes, Stack size 16 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_Start
  [Calls]
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> I2C_Delay
  [Called By]
  - >> DCMI_SingleRandomRead
  - >> DCMI_SingleRandomWrite
  - >> I2C_ReadByte

  I2C_Stop (Thumb, 46 bytes, Stack size 16 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_Stop
  [Calls]
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> I2C_Delay
  [Called By]
  - >> DCMI_SingleRandomRead
  - >> DCMI_SingleRandomWrite
  - >> I2C_ReadByte

  I2C_Ack (Thumb, 58 bytes, Stack size 16 bytes, i2c.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> I2C_Delay

  I2C_NoAck (Thumb, 58 bytes, Stack size 16 bytes, i2c.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> I2C_Delay
  [Called By]
  - >> I2C_ReadByte

  I2C_WaitAck (Thumb, 64 bytes, Stack size 16 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_WaitAck
  [Calls]
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> GPIO_ReadInputDataBit
  - >> I2C_Delay
  [Called By]
  - >> DCMI_SingleRandomRead
  - >> DCMI_SingleRandomWrite
  - >> I2C_ReadByte

  I2C_SendByte (Thumb, 78 bytes, Stack size 24 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = I2C_SendByte
  [Calls]
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> I2C_Delay
  [Called By]
  - >> DCMI_SingleRandomRead
  - >> DCMI_SingleRandomWrite
  - >> I2C_ReadByte

  I2C_ReceiveByte (Thumb, 96 bytes, Stack size 32 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = I2C_ReceiveByte
  [Calls]
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> GPIO_ReadInputDataBit
  - >> I2C_Delay
  [Called By]
  - >> DCMI_SingleRandomRead
  - >> I2C_ReadByte

  I2C_ReadByte (Thumb, 90 bytes, Stack size 16 bytes, i2c.o(.text), UNUSED)
  [Calls]

  - >> I2C_WaitAck
  - >> I2C_Stop
  - >> I2C_Start
  - >> I2C_SendByte
  - >> I2C_ReceiveByte
  - >> I2C_NoAck

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __fpl_dcmp_Inf (Thumb, 24 bytes, Stack size 0 bytes, dcmpi.o(x$fpl$dcmpinf), UNUSED)
  [Called By]

  - >> _dcmple

  __semihosting_library_function (Thumb, 0 bytes, Stack size 0 bytes, indicate_semi.o(.text), UNUSED)

  __aeabi_i2d (Thumb, 0 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dflt), UNUSED)
  [Called By]

  - >> LCD_FillPolyLine

  _dflt (Thumb, 46 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dflt), UNUSED)

  __aeabi_ui2d (Thumb, 0 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dfltu), UNUSED)
  [Called By]

  - >> LCD_FillPolyLine

  _dfltu (Thumb, 38 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dfltu), UNUSED)

  __aeabi_cdcmple (Thumb, 0 bytes, Stack size 32 bytes, dleqf.o(x$fpl$dleqf), UNUSED)
  [Called By]

  - >> LCD_FillPolyLine

  _dcmple (Thumb, 120 bytes, Stack size 32 bytes, dleqf.o(x$fpl$dleqf), UNUSED)
  [Calls]

  - >> __fpl_dnaninf
  - >> __fpl_dcmp_Inf

  __fpl_dcmple_InfNaN (Thumb, 0 bytes, Stack size unknown bytes, dleqf.o(x$fpl$dleqf), UNUSED)
  [Called By]

  - >> _drcmple

  __fpl_dnaninf (Thumb, 156 bytes, Stack size 16 bytes, dnaninf.o(x$fpl$dnaninf), UNUSED)
  [Called By]

  - >> _dcmple

  __aeabi_cdrcmple (Thumb, 0 bytes, Stack size 16 bytes, drleqf.o(x$fpl$drleqf), UNUSED)
  [Called By]

  - >> LCD_FillPolyLine

  _drcmple (Thumb, 108 bytes, Stack size 16 bytes, drleqf.o(x$fpl$drleqf), UNUSED)
  [Calls]

  - >> __fpl_dcmple_InfNaN

  _fp_init (Thumb, 10 bytes, Stack size 0 bytes, fpinit.o(x$fpl$fpinit))
  [Called By]

  - >> __rt_lib_init_fp_1

  __fplib_config_fpu_vfp (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  __fplib_config_pureend_doubles (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  ### Local Symbols

  SetSysClock (Thumb, 162 bytes, Stack size 12 bytes, system_stm32f4xx.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClock
  [Called By]
  - >> SystemInit

  LCD_PolyLineRelativeClosed (Thumb, 94 bytes, Stack size 28 bytes, stm3240f_lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_DrawLine
  [Called By]
  - >> LCD_ClosedPolyLineRelative
  - >> LCD_PolyLineRelative

  delay (Thumb, 22 bytes, Stack size 12 bytes, stm3240f_lcd.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = delay
  [Called By]
  - >> STM3240F_LCD_Init
  - >> LCD_PowerOn

  ### Undefined Global Symbols