CMSIS DSP Software Library: arm_lms_norm_init_q31.c Source File

- Main Page
- Modules
- Data Structures
- Files
- Examples

- File List
- Globals

# arm_lms_norm_init_q31.c

Go to the documentation of this file.

    00001 /*-----------------------------------------------------------------------------
    00002 * Copyright (C) 2010 ARM Limited. All rights reserved.
    00003 *
    00004 * $Date:        15. July 2011
    00005 * $Revision:    V1.0.10
    00006 *
    00007 * Project:      CMSIS DSP Library
    00008 * Title:        arm_lms_norm_init_q31.c
    00009 *
    00010 * Description:  Q31 NLMS initialization function.
    00011 *
    00012 * Target Processor: Cortex-M4/Cortex-M3/Cortex-M0
    00013 *
    00014 * Version 1.0.10 2011/7/15
    00015 *    Big Endian support added and Merged M0 and M3/M4 Source code.
    00016 *
    00017 * Version 1.0.3 2010/11/29
    00018 *    Re-organized the CMSIS folders and updated documentation.
    00019 *
    00020 * Version 1.0.2 2010/11/11
    00021 *    Documentation updated.
    00022 *
    00023 * Version 1.0.1 2010/10/05
    00024 *    Production release and review comments incorporated.
    00025 *
    00026 * Version 1.0.0 2010/09/20
    00027 *    Production release and review comments incorporated
    00028 *
    00029 * Version 0.0.7  2010/06/10
    00030 *    Misra-C changes done
    00031 * ---------------------------------------------------------------------------*/
    00032
    00033 #include "arm_math.h"
    00034 #include "arm_common_tables.h"
    00035
    00063 void arm_lms_norm_init_q31(
    00064   arm_lms_norm_instance_q31 * S,
    00065   uint16_t numTaps,
    00066   q31_t * pCoeffs,
    00067   q31_t * pState,
    00068   q31_t mu,
    00069   uint32_t blockSize,
    00070   uint8_t postShift)
    00071 {
    00072   /* Assign filter taps */
    00073   S->numTaps = numTaps;
    00074
    00075   /* Assign coefficient pointer */
    00076   S->pCoeffs = pCoeffs;
    00077
    00078   /* Clear state buffer and size is always blockSize + numTaps - 1  */
    00079   memset(pState, 0, (numTaps + (blockSize - 1u)) * sizeof(q31_t));
    00080
    00081   /* Assign post Shift value applied to coefficients */
    00082   S->postShift = postShift;
    00083
    00084   /* Assign state pointer */
    00085   S->pState = pState;
    00086
    00087   /* Assign Step size value */
    00088   S->mu = mu;
    00089
    00090   /* Initialize reciprocal pointer table */
    00091   S->recipTable = armRecipTableQ31;
    00092
    00093   /* Initialise Energy to zero */
    00094   S->energy = 0;
    00095
    00096   /* Initialise x0 to zero */
    00097   S->x0 = 0;
    00098
    00099 }
    00100

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines