CMSIS DSP Software Library: arm_fir_interpolate_f32.c Source File

- Main Page
- Modules
- Data Structures
- Files
- Examples

- File List
- Globals

# arm_fir_interpolate_f32.c

Go to the documentation of this file.

    00001 /* ----------------------------------------------------------------------
    00002 * Copyright (C) 2010 ARM Limited. All rights reserved.
    00003 *
    00004 * $Date:        15. July 2011
    00005 * $Revision:    V1.0.10
    00006 *
    00007 * Project:      CMSIS DSP Library
    00008 * Title:        arm_fir_interpolate_f32.c
    00009 *
    00010 * Description:  FIR interpolation for floating-point sequences.
    00011 *
    00012 * Target Processor: Cortex-M4/Cortex-M3/Cortex-M0
    00013 *
    00014 * Version 1.0.10 2011/7/15
    00015 *    Big Endian support added and Merged M0 and M3/M4 Source code.
    00016 *
    00017 * Version 1.0.3 2010/11/29
    00018 *    Re-organized the CMSIS folders and updated documentation.
    00019 *
    00020 * Version 1.0.2 2010/11/11
    00021 *    Documentation updated.
    00022 *
    00023 * Version 1.0.1 2010/10/05
    00024 *    Production release and review comments incorporated.
    00025 *
    00026 * Version 1.0.0 2010/09/20
    00027 *    Production release and review comments incorporated
    00028 *
    00029 * Version 0.0.7  2010/06/10
    00030 *    Misra-C changes done
    00031 * -------------------------------------------------------------------- */
    00032
    00033 #include "arm_math.h"
    00034
    00135 void arm_fir_interpolate_f32(
    00136   const arm_fir_interpolate_instance_f32 * S,
    00137   float32_t * pSrc,
    00138   float32_t * pDst,
    00139   uint32_t blockSize)
    00140 {
    00141   float32_t *pState = S->pState;                 /* State pointer */
    00142   float32_t *pCoeffs = S->pCoeffs;               /* Coefficient pointer */
    00143   float32_t *pStateCurnt;                        /* Points to the current sample of the state */
    00144   float32_t *ptr1, *ptr2;                        /* Temporary pointers for state and coefficient buffers */
    00145
    00146
    00147 #ifndef ARM_MATH_CM0
    00148
    00149   /* Run the below code for Cortex-M4 and Cortex-M3 */
    00150
    00151   float32_t sum0;                                /* Accumulators */
    00152   float32_t x0, c0;                              /* Temporary variables to hold state and coefficient values */
    00153   uint32_t i, blkCnt, j;                         /* Loop counters */
    00154   uint16_t phaseLen = S->phaseLength, tapCnt;    /* Length of each polyphase filter component */
    00155
    00156
    00157   /* S->pState buffer contains previous frame (phaseLen - 1) samples */
    00158   /* pStateCurnt points to the location where the new input data should be written */
    00159   pStateCurnt = S->pState + (phaseLen - 1u);
    00160
    00161   /* Total number of intput samples */
    00162   blkCnt = blockSize;
    00163
    00164   /* Loop over the blockSize. */
    00165   while(blkCnt > 0u)
    00166   {
    00167     /* Copy new input sample into the state buffer */
    00168     *pStateCurnt++ = *pSrc++;
    00169
    00170     /* Address modifier index of coefficient buffer */
    00171     j = 1u;
    00172
    00173     /* Loop over the Interpolation factor. */
    00174     i = S->L;
    00175     while(i > 0u)
    00176     {
    00177       /* Set accumulator to zero */
    00178       sum0 = 0.0f;
    00179
    00180       /* Initialize state pointer */
    00181       ptr1 = pState;
    00182
    00183       /* Initialize coefficient pointer */
    00184       ptr2 = pCoeffs + (S->L - j);
    00185
    00186       /* Loop over the polyPhase length. Unroll by a factor of 4.
    00187        ** Repeat until we've computed numTaps-(4*S->L) coefficients. */
    00188       tapCnt = phaseLen >> 2u;
    00189       while(tapCnt > 0u)
    00190       {
    00191
    00192         /* Read the coefficient */
    00193         c0 = *(ptr2);
    00194
    00195         /* Upsampling is done by stuffing L-1 zeros between each sample.
    00196          * So instead of multiplying zeros with coefficients,
    00197          * Increment the coefficient pointer by interpolation factor times. */
    00198         ptr2 += S->L;
    00199
    00200         /* Read the input sample */
    00201         x0 = *(ptr1++);
    00202
    00203         /* Perform the multiply-accumulate */
    00204         sum0 += x0 * c0;
    00205
    00206         /* Read the coefficient */
    00207         c0 = *(ptr2);
    00208
    00209         /* Increment the coefficient pointer by interpolation factor times. */
    00210         ptr2 += S->L;
    00211
    00212         /* Read the input sample */
    00213         x0 = *(ptr1++);
    00214
    00215         /* Perform the multiply-accumulate */
    00216         sum0 += x0 * c0;
    00217
    00218         /* Read the coefficient */
    00219         c0 = *(ptr2);
    00220
    00221         /* Increment the coefficient pointer by interpolation factor times. */
    00222         ptr2 += S->L;
    00223
    00224         /* Read the input sample */
    00225         x0 = *(ptr1++);
    00226
    00227         /* Perform the multiply-accumulate */
    00228         sum0 += x0 * c0;
    00229
    00230         /* Read the coefficient */
    00231         c0 = *(ptr2);
    00232
    00233         /* Increment the coefficient pointer by interpolation factor times. */
    00234         ptr2 += S->L;
    00235
    00236         /* Read the input sample */
    00237         x0 = *(ptr1++);
    00238
    00239         /* Perform the multiply-accumulate */
    00240         sum0 += x0 * c0;
    00241
    00242         /* Decrement the loop counter */
    00243         tapCnt--;
    00244       }
    00245
    00246       /* If the polyPhase length is not a multiple of 4, compute the remaining filter taps */
    00247       tapCnt = phaseLen % 0x4u;
    00248
    00249       while(tapCnt > 0u)
    00250       {
    00251         /* Perform the multiply-accumulate */
    00252         sum0 += *(ptr1++) * (*ptr2);
    00253
    00254         /* Increment the coefficient pointer by interpolation factor times. */
    00255         ptr2 += S->L;
    00256
    00257         /* Decrement the loop counter */
    00258         tapCnt--;
    00259       }
    00260
    00261       /* The result is in the accumulator, store in the destination buffer. */
    00262       *pDst++ = sum0;
    00263
    00264       /* Increment the address modifier index of coefficient buffer */
    00265       j++;
    00266
    00267       /* Decrement the loop counter */
    00268       i--;
    00269     }
    00270
    00271     /* Advance the state pointer by 1
    00272      * to process the next group of interpolation factor number samples */
    00273     pState = pState + 1;
    00274
    00275     /* Decrement the loop counter */
    00276     blkCnt--;
    00277   }
    00278
    00279   /* Processing is complete.
    00280    ** Now copy the last phaseLen - 1 samples to the satrt of the state buffer.
    00281    ** This prepares the state buffer for the next function call. */
    00282
    00283   /* Points to the start of the state buffer */
    00284   pStateCurnt = S->pState;
    00285
    00286   tapCnt = (phaseLen - 1u) >> 2u;
    00287
    00288   /* copy data */
    00289   while(tapCnt > 0u)
    00290   {
    00291     *pStateCurnt++ = *pState++;
    00292     *pStateCurnt++ = *pState++;
    00293     *pStateCurnt++ = *pState++;
    00294     *pStateCurnt++ = *pState++;
    00295
    00296     /* Decrement the loop counter */
    00297     tapCnt--;
    00298   }
    00299
    00300   tapCnt = (phaseLen - 1u) % 0x04u;
    00301
    00302   while(tapCnt > 0u)
    00303   {
    00304     *pStateCurnt++ = *pState++;
    00305
    00306     /* Decrement the loop counter */
    00307     tapCnt--;
    00308   }
    00309
    00310 #else
    00311
    00312   /* Run the below code for Cortex-M0 */
    00313
    00314   float32_t sum;                                 /* Accumulator */
    00315   uint32_t i, blkCnt;                            /* Loop counters */
    00316   uint16_t phaseLen = S->phaseLength, tapCnt;    /* Length of each polyphase filter component */
    00317
    00318
    00319   /* S->pState buffer contains previous frame (phaseLen - 1) samples */
    00320   /* pStateCurnt points to the location where the new input data should be written */
    00321   pStateCurnt = S->pState + (phaseLen - 1u);
    00322
    00323   /* Total number of intput samples */
    00324   blkCnt = blockSize;
    00325
    00326   /* Loop over the blockSize. */
    00327   while(blkCnt > 0u)
    00328   {
    00329     /* Copy new input sample into the state buffer */
    00330     *pStateCurnt++ = *pSrc++;
    00331
    00332     /* Loop over the Interpolation factor. */
    00333     i = S->L;
    00334
    00335     while(i > 0u)
    00336     {
    00337       /* Set accumulator to zero */
    00338       sum = 0.0f;
    00339
    00340       /* Initialize state pointer */
    00341       ptr1 = pState;
    00342
    00343       /* Initialize coefficient pointer */
    00344       ptr2 = pCoeffs + (i - 1u);
    00345
    00346       /* Loop over the polyPhase length */
    00347       tapCnt = phaseLen;
    00348
    00349       while(tapCnt > 0u)
    00350       {
    00351         /* Perform the multiply-accumulate */
    00352         sum += *ptr1++ * *ptr2;
    00353
    00354         /* Increment the coefficient pointer by interpolation factor times. */
    00355         ptr2 += S->L;
    00356
    00357         /* Decrement the loop counter */
    00358         tapCnt--;
    00359       }
    00360
    00361       /* The result is in the accumulator, store in the destination buffer. */
    00362       *pDst++ = sum;
    00363
    00364       /* Decrement the loop counter */
    00365       i--;
    00366     }
    00367
    00368     /* Advance the state pointer by 1
    00369      * to process the next group of interpolation factor number samples */
    00370     pState = pState + 1;
    00371
    00372     /* Decrement the loop counter */
    00373     blkCnt--;
    00374   }
    00375
    00376   /* Processing is complete.
    00377    ** Now copy the last phaseLen - 1 samples to the start of the state buffer.
    00378    ** This prepares the state buffer for the next function call. */
    00379
    00380   /* Points to the start of the state buffer */
    00381   pStateCurnt = S->pState;
    00382
    00383   tapCnt = phaseLen - 1u;
    00384
    00385   while(tapCnt > 0u)
    00386   {
    00387     *pStateCurnt++ = *pState++;
    00388
    00389     /* Decrement the loop counter */
    00390     tapCnt--;
    00391   }
    00392
    00393 #endif /*   #ifndef ARM_MATH_CM0 */
    00394
    00395 }
    00396

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines